# scipy.signal.iirnotch

scipy.signal.iirnotch(w0, Q, fs=2.0)

  Design second-order IIR notch digital filter.

  A notch filter is a band-stop filter with a narrow bandwidth (high quality factor). It rejects a narrow frequency band and leaves the rest of the spectrum little changed.

  Parameters:
    w0 float

      Frequency to remove from a signal. If fs is specified, this is in the same units as fs. By default, it is a normalized scalar that must satisfy `0 < w0 < 1`, with `w0 = 1` corresponding to half of the sampling frequency.

    Q float

      Quality factor. Dimensionless parameter that characterizes notch filter -3 dB bandwidth `bw` relative to its center frequency, `Q = w0/bw`.

    fs float, optional

      The sampling frequency of the digital system.

      New in version 1.2.0.

  Returns:
    b, a ndarray, ndarray

      Numerator (`b`) and denominator (`a`) polynomials of the IIR filter.

  See also

  `iirpeak`

  Notes

  New in version 0.19.0.

  References

  [1]

  Sophocles J. Orfanidis, “Introduction To Signal Processing”, Prentice-Hall, 1996

  Examples

  Design and plot filter to remove the 60 Hz component from a signal sampled at 200 Hz, using a quality factor Q = 30

      >>> from scipy import signal
      >>> import matplotlib.pyplot as plt
      >>> import numpy as np

      >>> fs = 200.0  # Sample frequency (Hz)
      >>> f0 = 60.0  # Frequency to be removed from signal (Hz)
      >>> Q = 30.0  # Quality factor
      >>> # Design notch filter
      >>> b, a = signal.iirnotch(f0, Q, fs)

      >>> # Frequency response
      >>> freq, h = signal.freqz(b, a, fs=fs)
      >>> # Plot
      >>> fig, ax = plt.subplots(2, 1, figsize=(8, 6))
      >>> ax[0].plot(freq, 20*np.log10(abs(h)), color='blue')
      >>> ax[0].set_title("Frequency Response")
      >>> ax[0].set_ylabel("Amplitude (dB)", color='blue')
      >>> ax[0].set_xlim([0, 100])
      >>> ax[0].set_ylim([-25, 10])
      >>> ax[0].grid(True)
      >>> ax[1].plot(freq, np.unwrap(np.angle(h))*180/np.pi, color='green')
      >>> ax[1].set_ylabel("Angle (degrees)", color='green')
      >>> ax[1].set_xlabel("Frequency (Hz)")
      >>> ax[1].set_xlim([0, 100])
      >>> ax[1].set_yticks([-90, -60, -30, 0, 30, 60, 90])
      >>> ax[1].set_ylim([-90, 90])
      >>> ax[1].grid(True)
      >>> plt.show()