# scipy.signal.check_COLA

scipy.signal.check_COLA(window, nperseg, noverlap, tol=1e-10)

  Check whether the Constant OverLap Add (COLA) constraint is met.

  Parameters:
    window str or tuple or array_like

      Desired window to use. If window is a string or tuple, it is passed to `get_window` to generate the window values, which are DFT-even by default. See `get_window` for a list of windows and required parameters. If window is array_like it will be used directly as the window and its length must be nperseg.

    nperseg int

      Length of each segment.

    noverlap int

      Number of points to overlap between segments.

    tol float, optional

      The allowed variance of a bin’s weighted sum from the median bin sum.

  Returns:
    verdict bool

      True if chosen combination satisfies COLA within tol, False otherwise

  See also

  `check_NOLA`

    Check whether the Nonzero Overlap Add (NOLA) constraint is met

  `stft`

    Short Time Fourier Transform

  `istft`

    Inverse Short Time Fourier Transform

  Notes

  In order to enable inversion of an STFT via the inverse STFT in `istft`, it is sufficient that the signal windowing obeys the constraint of “Constant OverLap Add” (COLA). This ensures that every point in the input data is equally weighted, thereby avoiding aliasing and allowing full reconstruction.

  Some examples of windows that satisfy COLA:

    - Rectangular window at overlap of 0, 1/2, 2/3, 3/4, …

    - Bartlett window at overlap of 1/2, 3/4, 5/6, …

    - Hann window at 1/2, 2/3, 3/4, …

    - Any Blackman family window at 2/3 overlap

    - Any window with `noverlap = nperseg-1`

  A very comprehensive list of other windows may be found in [2], wherein the COLA condition is satisfied when the “Amplitude Flatness” is unity.

  New in version 0.19.0.

  References

  [1]

  Julius O. Smith III, “Spectral Audio Signal Processing”, W3K Publishing, 2011,ISBN 978-0-9745607-3-1.

  [2]

  G. Heinzel, A. Ruediger and R. Schilling, “Spectrum and spectral density estimation by the Discrete Fourier transform (DFT), including a comprehensive list of window functions and some new at-top windows”, 2002, http://hdl.handle.net/11858/00-001M-0000-0013-557A-5

  Examples

      >>> from scipy import signal

  Confirm COLA condition for rectangular window of 75% (3/4) overlap:

      >>> signal.check_COLA(signal.windows.boxcar(100), 100, 75)
      True

  COLA is not true for 25% (1/4) overlap, though:

      >>> signal.check_COLA(signal.windows.boxcar(100), 100, 25)
      False

  “Symmetrical” Hann window (for filter design) is not COLA:

      >>> signal.check_COLA(signal.windows.hann(120, sym=True), 120, 60)
      False

  “Periodic” or “DFT-even” Hann window (for FFT analysis) is COLA for overlap of 1/2, 2/3, 3/4, etc.:

      >>> signal.check_COLA(signal.windows.hann(120, sym=False), 120, 60)
      True

      >>> signal.check_COLA(signal.windows.hann(120, sym=False), 120, 80)
      True

      >>> signal.check_COLA(signal.windows.hann(120, sym=False), 120, 90)
      True